REFRON – 32

(difluoromethane)

ANALYSIS:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S. No. | PARAMETRES | UNIT | SPECIFICATIONS (AS PER COLLABORATOR) | AVERAGE RESULTS |
| 1 | Moisture | Ppm (Max.) | 10 |  |
| 2 | Chloride as Cl- | Ppm (Max.) | NIL |  |
| 3 | Non-Volatile residue | Ppm (Max.) |  |  |
| 4 | Boiling range | oC (Max.) |  |  |
| 5 | Non-condensable gases | Vol. % (Max.) | 1.5 |  |
| 6 | Purity | % (Min.) | 99.95 |  |